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Purpose: 
Because we don’t know who or how many firefighters will respond to any specific alarm. This SOG outlines in priority who will Perform what tasks and what tools may be need to complete those tasks.  It is the responsibilities of the personnel riding to pre-determine job assignments prior to arrival using this list or of jobs. Senior members and ex-officers should assist in crew area.  The initial goal of the engine company is to place one hose line in operation with a water supply.

OBJECTIVE:  

The following guideline will describe the jobs / positions to be filled, the tools required and the order in which they are filled.  The officer in charge may deviate from as circumstances dictate. 

GUIDELIINE: 
Apparatus riding assignments are a type of “mini incident command system” for each responding apparatus. Listing the assignments on the fire apparatus simply guides what actions a firefighter will likely perform on the fireground.  

This system discourages freelancing and ensures accountability for all members operating on the fireground. 

Generally, the most important task for the first arriving engine will be to deploy the initial attack line and get water on the fire. Early control of the fire can make a safer environment for trapped occupants and fire department personnel. All members of the engine company should focus on this goal.

Riding positions for an Engine Company are as follows:

Engine
1 - Driver/Operator
2 - Officer/OIC 
3 - Nozzle
4 - Back up/hydrant supply

5 - Door / control


Position #1- (Driver / Operator) 
1. Responsible for safely transporting firefighting personnel to and from an emergency scene. 

2. Responsible for laying supply lines and making supply line connections to apparatus and coordinating with the second due engine.
3. Responsible for operating pump/providing scene lighting and equipment accountability. 

4. Tools: 

a. Appropriate clothing / Safety vest
b. Portable radio monitoring appropriate Response and Operations Channels at all times.
Position #2-(Officer/OIC) 
1. Initial size up and serves as initial IC if  required
2. Supervises and assists when needed with hose line management, forcible entry, initial fire attack and accountability. (especially in three man crew) 
3. Establish interior sector command, monitors conditions, makes periodic reports concerning conditions and needs to Command. 
4. Tools: 

a. Full Turnout Gear w/SCBA 

b. Portable radio 

c. Flashlight

d. Thermal Imager
e. Small tool (Irons or hook) 

Position #3-(Nozzle man) 
1. Pulls appropriate hand line according to WFD SOG’s for the type of fire, Grasping nozzle and first fold.  Lays out line to facilitate rapid advancement, bleeds air from line and assures proper stream pattern before entry.
2. Performs initial fire attack, confine and extinguish fire, as well as search & rescue, ventilation, and overhaul as required by the conditions of the incident. 
3.  Brings water can for alarms
3.  Tools: 

a. Full Turnout Gear w/SCBA 

b. Portable Radio 

c. Flashlight

d. Appropriate size attack line & nozzle / Water can

If only 3 firefighters are available, this position will be responsible for the layout of the supply line. Once the hydrant wrap is made, the firefighter will re-mount the apparatus and continue to the fire scene to carry out duties.
Position #4 (Hydrant man) 
1. Exits apparatus at hydrant with necessary tools to establish water supply. 

2. Efficiently makes hydrant connection and a wait’s the Driver / operators command to charge the hydrant. 

3. After water supply has been established, returns to the Engine, picks up tools and becomes back up man in a 4 person crew,  In 5 person crew he will become contol  position or reports to the interior sector command for assignment. 
4.  Assist with advancement of attack line. 
5.  Tools: 

a. Full Turnout Gear w/SCBA 

b. Portable Radio

c. Flashlight 

d. Hydrant valve, adapter, wrenches and enough hose to wrap hydrant. 
Upon sounding of the portable air horn (3 blasts) by the driver, the hydrant will be opened completely, if radio is available the driver will radio for hydrant to be opened.  Once the water is flowing, proceed to the fire ground.  With four member crew he then assumes position #5 at this point or next available position not filled. 

Position #5 Back-up
1. Grab second fold and assist w/Stretch of attack line (flake out and remove kinks),
2. Forcible entry if needed.
3. Back-up Nozzle man on the initial attack line 
4. Tools: 

a. Full Turnout Gear 

b. Portable radio 
c. Flashlight

d. Flat head axe & Halligan tool (Irons)
Position #6 (Door / Second line Nozzle man) 
1.  Assist initial hose team with advancement in long stretches

2.  Remains at door to help feed hose and monitor fire conditions

3.  Nozzle man of second line at car fires. 

4.  Pulls second suitable hose line for back-up job. 
5.  Tools: 

a. Full Turnout Gear 

b. Portable radio 

c. Flashlight

d. Hook 

e. Nozzle

Note: This position applies with full staffing ONLY
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