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PURPOSE: 
This guideline sets the standard for storage of all Wyckoff Fire Department Engine pumps. 

OBJECTIVE: 
This is to keep all pumps in the department set the same for the ease of the chauffeurs.

GUIDELINE:  
All Wyckoff Fire Department engines’ pumps will be stored wet, that is with the tank to pump gate open.
Engines equipped with a relief valve will be stored with the valve turned off and preset to 130 psi.
Engines equipped with a pressure governor will be preset to 130 psi.

When equipped with a transfer valve it will be stored in the pressure mode.
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