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PURPOSE: 
To make it easy for everyone to be familiar with the amount of hose and method of deployment for all supply lines carried and used on all Wyckoff Fire Department Engines. 

OBJECTIVE: 
To provide standards of storage and method of deployment so that all other firefighters are aware of what will be happening and can plan their actions accordingly. This guideline will also provide standards of what is expected in regards to repacking and setting up for future operations.
GUIDELINE:   
· Five inch supply line will be used for all water supply and tower operations. All supply line will be flat packed in the center rear beds with all couplings staggered to the front of hose bed so not to flip on deployment. There will be a minimum, of twelve (1200) hundred feet of supply line with at least two twenty five (25) foot ponies on each engine.

· When dropping the line, the line will be laid on the same side of the street as the hydrant used. If the address is on the opposite side as hydrant hit, the engine will lay line on the same side as hydrant. Once past the address, the engine may cross over going to first due engine positioning. The hydrassist valve will be used whenever possible for connecting supply line to hydrant. 

· The hydrassist valve will be stored at the rear of the apparatus connected to five inch supply line. A hydrant wrench will be stored on the valve.

· The intake valve used in supply line operations will be mounted on the officer’s side steamer connection on all engines within the Wyckoff Fire Department. The air bleeder valve on the intake will be stored in the open position. 
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