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PURPOSE: 
The setting of standards and requirements for preconnected and packed hose beds will allow all members to be familiar and comfortable with any engine in the Wyckoff Fire Department.
OBJECTIVE: 
This guideline will set the standards which will be used for all Wyckoff Fire 
Department engines for the packing and deployment of attack lines.
GUIDELINE:  
1 Motor Vehicle Fire Attack Lines

· There will be two 1 ¾” lines dedicated to use for car fires.

· Each will be 150’-200’ in length.

· One line will be preconnected and set up with a fog nozzle.
· One line will be preconnected and set up with a bent tip applicator.

· Car beds are typically set up in the crosslay positions. Any exceptions will need to be approved by the board of fire officers. (currently eng 236 is at side of rear hose bed)
2 House Fire Attack Lines
· There will be two 1 ¾” lines dedicated to use for residential structure fires.

· Each will be a minimum of 250’ in length

· One line will be preconnected and set up with an adjustable fog nozzle preset to 125 GPM per WFD SOG 402.3.6.

· One line will be preconnected and set up with a smooth bore nozzle.

· House beds are typically set up on the side of the rear hose bed. Any exceptions will need to be approved by the board of fire officers. (currently eng 236 is at crosslay position)

· Smoothbore nozzles will be used on the inside bed and fog nozzles will be used on the outside bed.

3 High Rise Packs
· All first due engines will carry a high rise pack.

· A high rise pack will consist of  200’ of  1 ¾” hose either all joined or in two sections of 100’.

· The hose will be bundled in such a way as to make it easy to carry to a remote location for use.
4 High Rise Equipment Bag

· All of this equipment should be stored on the engine in a bag and should be known as the High Rise Equipment Bag. This bag should contain but not limited to the following: Gated wye, spanner wrench, fog nozzle, hydrant wrench or pipe wrench and couplings or adapters.
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