SOG 402.3.11-Attack Line Selection
Revision: 7/27/09

[image: image2.jpg]



[image: image1]
PURPOSE: 
To provide standard terminology and thus eliminate confusion on the fireground while attempting to reach longer distances than can be reached with preconnected hoses.
OBJECTIVE: 
The objective of this guideline is to set standard terminology of a simple nature that allows everyone to understand what lengths and sizes of hose will be used.
GUIDELINE:  
To minimize confusion and ease the officer’s burden of accomplishing a hose line stretch at long or questionable distances, a simple standard terminology shall be adopted.  The officer or individual in Command will use a two number command.  The first number will indicate the amount in feet of supply line to be stretched with a gated wye attached.  The second number will indicate the amount of line that will be attached at the wye.

Example: “Do an extended lay, two fifty and one fifty.”
     Will mean 250’ of supply (typically 3”) with a 150’ length of attack line (typically 1 ¾”) attached. Larger or smaller sized hose can be designated by the officer.
The second attack line should not be specified during the initial set up.  This will allow easier and faster set up and also determine if sufficient length was called for. 
Each first due engine in the Wyckoff Fire Department is required to carry at least 250’ of 3” supply line that is packed as a single lay on a rear bed. 
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