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PURPOSE: 
All Members of the Wyckoff Fire Department must follow certain procedures in order to avoid exposure to certain dangers involved with motor vehicle fires.
OBJECTIVE: 
This guideline provides the goals and procedures for attacking a motor vehicle fire. 
GUIDELINE:
1. Auto fire attacks shall consist of a minimum of two attack lines.
· The first line is for the direct fire attack.  This line will be equipped with an adjustable fog nozzle. The vehicle should be approached from a 45° angle to avoid any possible projectiles from gas charged piston explosions, etc.
· The second will be dedicated to the protection of the fuel supply and storage system.  It will be equipped with a nozzle of the bent tip applicator type. Approach to the vehicle should also be made from a 45° angle.
· All members involved in the fire attack should be in full PPE and utilizing an SCBA.

2. As in all motor vehicle incidents the vehicle should be stabilized and the battery disconnected as soon as possible.

3. Once the fire has been knocked down firefighters should always check to confirm that the vehicle was not occupied.  This includes a check of any sealed compartments such as the vehicle trunk.  
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