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PURPOSE: 
To set a standard for all apparatus nozzle storage.
OBJECTIVE: 
This guideline is designed to allow all members to be familiar with the settings of all adjustable nozzles on all apparatus of the Wyckoff Fire Department.
GUIDELINE:   
On all Wyckoff Fire Department apparatus the adjustable nozzles will be stored as follows:

1 ½” 
95 gpm

1 ¾”
125 gpm

2 ½”
250 gpm
All adjustable nozzles will be stored to provide a straight stream upon opening.
All nozzles will be stored in the closed position.
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